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Elf is a 12 foot long, 5 foot beam, vee bottom sailing or rowing boat. The waterlines shown are at 300 lbs and 500 lbs. The bare hull should run in the 60-90lb range, depending on thickness of ply used.  She should make a nice family rower or 2-3 person daysailer.  Seating and rigging arrangements are up to the builder.  Construction is of Stitch and glue.

	Bottom Panel

	Station
	X
	Y
	X2
	Y2

	1
	N/A
	N/A
	0
	17 11/16"

	2
	5/8"
	1 1/16"
	 
	 

	3
	12"
	3/4"
	12"
	20"

	4
	24"
	7/16"
	24"
	21 7/8"

	5
	36"
	3/16"
	36"
	23 1/8"

	6
	48"
	1/16"
	48"
	23 3/4"

	7
	60"
	0"
	60"
	24"

	8
	72"
	0"
	72"
	23 3/4"

	9
	84"
	1/16"
	84"
	22 3/16"

	10
	96"
	3/16"
	96"
	19 3/4"

	11
	108"
	1/2"
	108"
	15 1/4"

	12
	120"
	1"
	120"
	10 5/8"

	13
	132"
	2 1/8" 
	132"
	4 1/16"

	14
	135 7/16"
	2 1/2"
	135 7/16"
	2 1/2"

	

	Side Panels

	Station
	X
	Y
	X2
	Y2

	1
	N/A
	N/A
	0"
	11"

	2
	2 5/8"
	0
	 
	 

	3
	12"
	5/16"
	12"
	12 1/4"

	4
	24"
	7/16"
	24"
	13 1/2"

	5
	36"
	1/2"
	36"
	14 1/2"

	6
	48"
	9/16"
	48"
	15 1/2"

	7
	60"
	1"
	60"
	16 1/4"

	8
	72"
	1 3/8"
	72"
	16 13/16"

	9
	84"
	1 15/16"
	84"
	17 1/4"

	10
	96"
	2"
	96"
	17 5/16"

	11
	108"
	1 13/16"
	108"
	17 3/16"

	12
	120"
	1 3/8"
	120"
	16 3/4"

	13
	132"
	5/8"
	132"
	16 1/8"

	14
	141 5/8"
	0"
	 
	 

	15
	144"
	0"
	144"
	15 1/8"

	16
	152 1/8"
	0"
	152 1/8"
	14 3/4"

	 

	Transom
	
	

	Station
	X
	Y
	
	

	1
	0"
	0"
	
	

	2
	3"
	16 3/8"
	
	

	3
	13 1/2"
	20 1/2"
	
	


All measurements are in inches. The end points of the plotted lines are joined by a straight line.
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This shows how the measurements are used to lay out the panels. X and Y are the bottom line of the panel and X2 and Y2 are the top line. All points are from the edge of the ply or a baseline. Any points which are N/A are not plotted. They may just be not on the panel or are not important to that line. The two end points are closed with a straight line.

For information on Stitch and Glue, please check the construction of fisher10. The hull was done entirely with stitch and glue, except for the transom/side panel joint, which was first attached with screws and then filleted on the inside and taped on the outside. There are also many good sites with Stitch and glue information. www.bateau.com has an excellent primer on the subject, so do most of the other major plans dealers, such as Glenn-L and Clark Craft. 

