Figure 2.5 Resistance Measurement with an Oscilloscope. This figure shows a stylized drawing of an oscilloscope and schematic symbols of resistors. The scope has a CAL, calibrator, output and a single input V IN, vertical input. The hot side of the CAL output goes through a resistor, RX then another resistor, RR, to the scope ground. The junction of the two resistors goes to the hot terminal of the V IN connector. This completes the verbal description.
Go back