BeSweet v1.4
BeLight v0.2.2.0 beta 8

Program Description:

BeSweet allows a direct conversion from AC3/MPA/MP2/MP3/WAV/LPCM/VOB to WAV/MP2/MP3/OGG/AIFF/AC3 and also WaveMP3 & Dolby-Digital-WAV. The output product can be customized using many many switches.
 
BeLight is a Graphical User Interface (GUI) for BeSweet.

Features:
 
- BeLight supports as Input files:
  AC3, MP2, MP3, MPA, OGG, VORBIS, WAV, AVI, VOB, LST & MUX
- BeLight supports as Output Formats:
  AAC/MP4, AC3, AIFF, MP2, MP3, VORBIS & WAV 
- Provides the most BeSweet functions
  Gain, SSRC, Boost, Change Frame Rate, Soundtouch & Partial Encoding
- Plugins Support
- Presets
- Shibatch Equalizer. 
- Delay Detection from the input filename
- MultiLanguages Support
  German, Spanish, English and French

Minimum Requirements:

- Windows 98

Installation Instructions:

1.) Copy the "BeSweet v1.4" folder wherever you want on your hard drive.
2.) Make a shortcut to "BeLight.exe" in the "BeSweet v1.4" folder on your desktop.
3.) Run "BeLight.exe" in the "BeSweet v1.4" folder and follow the instructions.

If you enjoy the software and use it, make a donation to support the software developers.