Figure 8.14. Inputs eh and b feed into gate 2 which is an AND gate. Input B feeds into an inverter which is numbered 1 and is a not function. The term not gate is never used. Input D feeds into gate 3 which is an AND gate. The output of the inverter feeds the other input of gate 3. The outputs of gates 2 and 3 feed into gate 4 which is an or gate. The output of gate 4 is the variable P. End verbal description.
Go back.