Figure 1.8. On the left the battery labeled E1 has been removed and replaced by a short circuit, a piece of wire, a line. The left end of a resistor, R1 = 240 ohms, connects to the bottom line. The right end of R1 is connected to the top end of R2 = 400 ohms. The bottom end of R2 is connected to the bottom line. The junction of R1 and R2 connects to the left end of R3 = 350 ohms. E2 is also replaced by a short circuit. The right end of R3 connects to the top end of R4 = 750 ohms. The bottom of R4 connects to the bottom line. The junction of R3 and R4 connects to the left end of R5 = 100 ohms. The right end of R5 connects to the upper output terminal. The lower output terminal connects to the bottom line of the circuit. End verbal description.
Go back.