Figure 1.16. On the left is a battery labeled E = 30 v. The bottom, negative, end is connected to the bottom line of the circuit. The top, positive, end connects to the left end of a resistor labeled R1 = 2 k ohms. The right end of R1 connects to the top of another resistor labeled R2 = 1 k ohm. The bottom end of R2 connects to the bottom line. The lower output terminal connects to the bottom line. The upper output terminal connects to the junction of R1 and R2. End verbal description.
Go back.