Figure 1.15. On the left is an ideal current source. The arrow is pointing up. The current source is labeled I N = 23.636 mA. The bottom end of I N is connected to the bottom line of the circuit. The upper end is connected to the top end of a resistor labeled R N = 76.744 ohms. The lower end of R N is connected to the bottom line. The upper output terminal is connected to the top of I N and R N. The lower terminal is connected to the bottom line. There is a resistor connected across the terminals. It is labeled R2 = 75 ohms. End verbal description.
Go back.