Figure 6.4. The upper input terminal connects through a resistor labeled R1, to the inverting input of an op amp. The lower input terminal is grounded. The output of the op amp connects through a resistor labeled R2, to the inverting input. The noninverting input is grounded. The output of the op amp goes to the upper output terminal. The lower output terminal is grounded. End verbal description.
Go back.