By now you should have this one down cold. The center tapped transformer winding connects to the anodes of the two diodes and CT to ground. The diode cathodes connect to the positive end of a 1000 mu f cap. This point connects through a 24 ohm 1 watt res to the positive end of another 1000 mu f cap. The negative ends of both caps are grounded. The positive end of the second cap connects to pin 4, heater, of a 12AX7. Pin 5 is grounded. End verbal description.
go back.