Figure 1.11. On the left an ideal voltage source is labeled V Th = 1.814 v. The lower, positive end, connects to the bottom line of the circuit. The top, negative end, of V Th connects to the left end of a resistor labeled R Th = 76.74 ohms. The right end of R Th connects to the top output terminal. The bottom line connects to the lower output terminal. There is a resistor connected across the two output terminals. It is labeled R2 = 75 ohms. End verbal description.
Go back.