Figure 1.24. There are two terminals on the left. The upper terminal connects to the left end of a resistor labeled R V. The right end of R V connects to the left end of another resistor which is labeled with a value, 98.2 k ohms. The right end of this resistor connects to the upper, positive end, of a microamp meter. The other end of the meter connects to the lower terminal. The meter is labeled I M = 50 microamps, R M = 1800 ohms. End verbal description.
Go back.