Figure 3eh.6. This is a graph. The horizontal axis is labeled plate voltage in volts and goes from 0 to 100 with numbered marks every 20 volts and minor marks every 4 volts. The vertical scale is labeled Plate current in mA and goes from 0 to 1600 with numbered marks every 200 mA and minor marks every 50 mA. The curve starts out at the point 0,0 and subsequent points will be given as voltage followed by current with a comma between. 0, 0. 20, 130. 40, 350. 60, 700. 80, 1,075. 100, 1,475. End verbal description.
Go back.