Figure 6.12 Emitter-follower with Base to Emitter Short. Plus 12 volts is at the top of the diagram and ground is at the bottom. A resistor, R1, 10 k ohms,, has one end connected to plus 12 volts. The other end connects to a point we will call X. Point X also connects to another resistor, R2, 22 k ohms. The other end of R2 goes to ground. Point X also connects to one end of a capacitor. The other endof the capacitor connects to a connection terminal. Another connection terminal goes to ground. Together, these two terminals are labeled input. Another resistor, R E, 4.7 k ohms, has one end connected to ground. The other end connects to point X. point X also connects to one end of another capacitor. The other end of the capacitor connects to a terminal. Another terminal goes to ground. Together, these two terminals are labeled output. End verbal description.
Go back.