Figure 0.8, Transistor with Constant Voltage Biasing. There is a battery labeled V sub CC. The negative end is connected to common. The positive end goes to one end of a resistor, R1. The other end of R1 goes to the base of an N P N transistor. The base also goes to one end of another resistor labeled R2. The other end of R2 goes to common. The positive end of V sub CC also goes to another resistor labeled R sub C. The other end of R sub C goes to the collector of the transistor. The emitter of the transistor goes to one end of R sub E. The other end of R sub E goes to common. This completes the verbal description.
Go back.