Figure 6.9 Emitter-Follower with Shorted NPN BJT. Plus 12 volts is at the top of the diagram and ground is at the bottom. A resistor, R1, has one end connected to plus 12 volts. The other end connects to the anode of a diode. R1 also connects to another resistor, R2. The other end of R2 goes to ground. The junction of R1 and R2 also connect to the top end of R E. The other end of R E goes to ground. The cathode of the diode connects to plus 12 volts. End verbal description.
Go back.