Figure 6.8 Emitter-Follower Circuit. Plus 12 volts is at the top of the diagram and ground is at the bottom. A resistor, R1, has one end connected to plus 12 volts. The other end connects to the base of an N P N bipolar junction transistor, BJT. The base also connects to another resistor, R2. The other end of R2 goes to ground. The collector connects to plus 12 volts. Another resistor, R E, has one end connected to ground. The other end connects to the emitter of the transistor. End verbal description.
Go back.