Figure 6.7. The upper input terminal goes through a resistor labeled R to the inverting input of an op amp. The lower input terminal and the noninverting input are grounded. The output connects through a capacitor labeled C to the inverting input. There is a switch in parallel with the capacitor. The output of the op amp goes to the upper output terminal of the circuit. The lower output terminal is grounded. End verbal description.
Go back.