Figure 8.33. Pins 8 and 4 are tied together and go to plus 12 volts. pin 1 is grounded. There is a .01 u f capacitor connected from pin 5 to ground. There is a resistor, R1, from plus 12 volts to pin 7. There is another resistor, R2, from pin 7 to pin 6. There is a capacitor, C, from pin 6 to ground. Pin 6 is tied to pin 2. Pin 3, output, is not shown connected to anything. End verbal description.
Go back.